<map id="BNO08x::calibrate_accelerometer" name="BNO08x::calibrate_accelerometer">
<area shape="rect" id="Node000001" title="Sends command to calibrate accelerometer." alt="" coords="5,43,222,69"/>
<area shape="rect" id="Node000002" href="$class_b_n_o08x.html#ad097849616c5caab1fd3eb3632ee2b91" title="Queues a packet containing a command to calibrate the specified sensor." alt="" coords="273,5,442,48"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="222,40,257,36,258,41,222,46"/>
<area shape="rect" id="Node000005" href="$class_b_n_o08x.html#a7cdeb849e728487de961cdfd4030c773" title="Waits for a queued packet to be sent or host_int_timeout_ms to elapse." alt="" coords="270,72,445,99"/>
<area shape="poly" id="edge4_Node000001_Node000005" title=" " alt="" coords="222,66,254,70,253,76,222,72"/>
<area shape="rect" id="Node000003" href="$class_b_n_o08x.html#a5cc58139e4d5f0587b90e249ceb476f9" title="Queues a packet containing a command." alt="" coords="493,13,670,40"/>
<area shape="poly" id="edge2_Node000002_Node000003" title=" " alt="" coords="442,24,477,24,477,29,442,29"/>
<area shape="rect" id="Node000004" href="$class_b_n_o08x.html#a62c570ba96512f4d0d10b2594048de1f" title="Queues an SHTP packet to be sent via SPI." alt="" coords="718,13,878,40"/>
<area shape="poly" id="edge3_Node000003_Node000004" title=" " alt="" coords="671,24,703,24,703,29,671,29"/>
</map>
