<map id="BNO08x::enable_ARVR_stabilized_rotation_vector" name="BNO08x::enable_ARVR_stabilized_rotation_vector">
<area shape="rect" id="Node000001" title="Sends command to enable ARVR stabilized rotation vector reports (See Ref. Manual 6...." alt="" coords="5,80,165,139"/>
<area shape="rect" id="Node000002" href="$class_b_n_o08x.html#a41613e65ea9beef883184b7ef67affdd" title="Enables a sensor report for a given ID." alt="" coords="213,96,369,123"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="165,107,197,107,197,112,165,112"/>
<area shape="rect" id="Node000003" href="$class_b_n_o08x.html#af2951f6ea448af7cf7932fbfed9fec3c" title="Queues a packet containing a command with a request for sensor reports, reported periodically...." alt="" coords="425,29,584,72"/>
<area shape="poly" id="edge2_Node000002_Node000003" title=" " alt="" coords="341,93,409,74,411,79,343,98"/>
<area shape="rect" id="Node000004" href="$class_b_n_o08x.html#a2897a178bf2c53cd99df0d4570edf72e" title="Waits for data to be received over SPI, or HOST_INT_TIMEOUT_MS to elapse." alt="" coords="417,96,592,123"/>
<area shape="poly" id="edge4_Node000002_Node000004" title=" " alt="" coords="370,107,402,107,402,112,370,112"/>
<area shape="rect" id="Node000005" href="$class_b_n_o08x.html#a7cdeb849e728487de961cdfd4030c773" title="Waits for a queued packet to be sent or HOST_INT_TIMEOUT_MS to elapse." alt="" coords="417,147,592,173"/>
<area shape="poly" id="edge5_Node000002_Node000005" title=" " alt="" coords="351,121,431,140,430,145,350,126"/>
<area shape="poly" id="edge3_Node000003_Node000003" title=" " alt="" coords="464,29,462,19,469,10,483,5,505,3,528,5,541,11,539,16,526,10,505,8,485,10,472,15,467,21,469,28"/>
</map>
