<map id="BNO08x::enable_linear_accelerometer" name="BNO08x::enable_linear_accelerometer">
<area shape="rect" id="Node000001" title="Sends command to enable linear accelerometer reports (See Ref. Manual 6.5.10)" alt="" coords="5,88,160,131"/>
<area shape="rect" id="Node000002" href="$class_b_n_o08x.html#a41613e65ea9beef883184b7ef67affdd" title="Enables a sensor report for a given ID." alt="" coords="208,96,364,123"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="160,107,193,107,193,112,160,112"/>
<area shape="rect" id="Node000003" href="$class_b_n_o08x.html#af2951f6ea448af7cf7932fbfed9fec3c" title="Queues a packet containing a command with a request for sensor reports, reported periodically...." alt="" coords="420,29,579,72"/>
<area shape="poly" id="edge2_Node000002_Node000003" title=" " alt="" coords="336,93,404,74,406,79,338,98"/>
<area shape="rect" id="Node000004" href="$class_b_n_o08x.html#a2897a178bf2c53cd99df0d4570edf72e" title="Waits for data to be received over SPI, or HOST_INT_TIMEOUT_MS to elapse." alt="" coords="412,96,587,123"/>
<area shape="poly" id="edge4_Node000002_Node000004" title=" " alt="" coords="365,107,397,107,397,112,365,112"/>
<area shape="rect" id="Node000005" href="$class_b_n_o08x.html#a7cdeb849e728487de961cdfd4030c773" title="Waits for a queued packet to be sent or HOST_INT_TIMEOUT_MS to elapse." alt="" coords="412,147,587,173"/>
<area shape="poly" id="edge5_Node000002_Node000005" title=" " alt="" coords="346,121,426,140,425,145,345,126"/>
<area shape="poly" id="edge3_Node000003_Node000003" title=" " alt="" coords="459,29,457,19,464,10,478,5,500,3,523,5,536,11,534,16,521,10,500,8,480,10,467,15,462,21,464,28"/>
</map>
