<map id="BNO08x::enable_activity_classifier" name="BNO08x::enable_activity_classifier">
<area shape="rect" id="Node000001" title="Sends command to enable activity classifier reports (See Ref. Manual 6.5.36)" alt="" coords="5,88,169,131"/>
<area shape="rect" id="Node000002" href="$class_b_n_o08x.html#a41613e65ea9beef883184b7ef67affdd" title="Enables a sensor report for a given ID." alt="" coords="217,96,373,123"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="169,107,201,107,201,112,169,112"/>
<area shape="rect" id="Node000003" href="$class_b_n_o08x.html#af2951f6ea448af7cf7932fbfed9fec3c" title="Queues a packet containing a command with a request for sensor reports, reported periodically...." alt="" coords="429,29,588,72"/>
<area shape="poly" id="edge2_Node000002_Node000003" title=" " alt="" coords="345,93,413,74,415,79,347,98"/>
<area shape="rect" id="Node000004" href="$class_b_n_o08x.html#a2897a178bf2c53cd99df0d4570edf72e" title="Waits for data to be received over SPI, or HOST_INT_TIMEOUT_MS to elapse." alt="" coords="421,96,596,123"/>
<area shape="poly" id="edge4_Node000002_Node000004" title=" " alt="" coords="374,107,406,107,406,112,374,112"/>
<area shape="rect" id="Node000005" href="$class_b_n_o08x.html#a7cdeb849e728487de961cdfd4030c773" title="Waits for a queued packet to be sent or HOST_INT_TIMEOUT_MS to elapse." alt="" coords="421,147,596,173"/>
<area shape="poly" id="edge5_Node000002_Node000005" title=" " alt="" coords="355,121,435,140,434,145,354,126"/>
<area shape="poly" id="edge3_Node000003_Node000003" title=" " alt="" coords="468,29,466,19,473,10,487,5,509,3,532,5,545,11,543,16,530,10,509,8,489,10,476,15,471,21,473,28"/>
</map>
