<map id="BNO08x::enable_report" name="BNO08x::enable_report">
<area shape="rect" id="Node000001" title="Enables a sensor report for a given ID." alt="" coords="5,96,162,123"/>
<area shape="rect" id="Node000002" href="$class_b_n_o08x.html#af2951f6ea448af7cf7932fbfed9fec3c" title="Queues a packet containing a command with a request for sensor reports, reported periodically...." alt="" coords="218,29,377,72"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="134,93,202,74,203,79,136,98"/>
<area shape="rect" id="Node000003" href="$class_b_n_o08x.html#a2897a178bf2c53cd99df0d4570edf72e" title="Waits for data to be received over SPI, or HOST_INT_TIMEOUT_MS to elapse." alt="" coords="210,96,385,123"/>
<area shape="poly" id="edge3_Node000001_Node000003" title=" " alt="" coords="162,107,194,107,194,112,162,112"/>
<area shape="rect" id="Node000004" href="$class_b_n_o08x.html#a7cdeb849e728487de961cdfd4030c773" title="Waits for a queued packet to be sent or HOST_INT_TIMEOUT_MS to elapse." alt="" coords="210,147,385,173"/>
<area shape="poly" id="edge4_Node000001_Node000004" title=" " alt="" coords="144,121,224,140,223,145,142,126"/>
<area shape="poly" id="edge2_Node000002_Node000002" title=" " alt="" coords="257,29,255,19,262,10,276,5,297,3,320,5,334,11,332,16,319,10,297,8,277,10,265,15,260,21,262,28"/>
</map>
