<map id="BNO08x::enable_tap_detector" name="BNO08x::enable_tap_detector">
<area shape="rect" id="Node000001" title="Sends command to enable tap detector reports (See Ref. Manual 6.5.27)" alt="" coords="5,88,147,131"/>
<area shape="rect" id="Node000002" href="$class_b_n_o08x.html#a41613e65ea9beef883184b7ef67affdd" title="Enables a sensor report for a given ID." alt="" coords="195,96,351,123"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="147,107,179,107,179,112,147,112"/>
<area shape="rect" id="Node000003" href="$class_b_n_o08x.html#af2951f6ea448af7cf7932fbfed9fec3c" title="Queues a packet containing a command with a request for sensor reports, reported periodically...." alt="" coords="407,29,566,72"/>
<area shape="poly" id="edge2_Node000002_Node000003" title=" " alt="" coords="323,93,391,74,393,79,325,98"/>
<area shape="rect" id="Node000004" href="$class_b_n_o08x.html#a2897a178bf2c53cd99df0d4570edf72e" title="Waits for data to be received over SPI, or HOST_INT_TIMEOUT_MS to elapse." alt="" coords="399,96,574,123"/>
<area shape="poly" id="edge4_Node000002_Node000004" title=" " alt="" coords="352,107,384,107,384,112,352,112"/>
<area shape="rect" id="Node000005" href="$class_b_n_o08x.html#a7cdeb849e728487de961cdfd4030c773" title="Waits for a queued packet to be sent or HOST_INT_TIMEOUT_MS to elapse." alt="" coords="399,147,574,173"/>
<area shape="poly" id="edge5_Node000002_Node000005" title=" " alt="" coords="333,121,413,140,412,145,332,126"/>
<area shape="poly" id="edge3_Node000003_Node000003" title=" " alt="" coords="446,29,444,19,451,10,465,5,487,3,510,5,523,11,521,16,508,10,487,8,467,10,454,15,449,21,451,28"/>
</map>
