<map id="BNO08x::calibrate_planar_accelerometer" name="BNO08x::calibrate_planar_accelerometer">
<area shape="rect" id="Node000001" title="Sends command to calibrate planar accelerometer." alt="" coords="5,35,175,77"/>
<area shape="rect" id="Node000002" href="$class_b_n_o08x.html#ad097849616c5caab1fd3eb3632ee2b91" title="Queues a packet containing a command to calibrate the specified sensor." alt="" coords="226,5,395,48"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="175,42,210,37,211,43,175,47"/>
<area shape="rect" id="Node000005" href="$class_b_n_o08x.html#a7cdeb849e728487de961cdfd4030c773" title="Waits for a queued packet to be sent or HOST_INT_TIMEOUT_MS to elapse." alt="" coords="223,72,398,99"/>
<area shape="poly" id="edge4_Node000001_Node000005" title=" " alt="" coords="175,65,207,69,207,74,175,70"/>
<area shape="rect" id="Node000003" href="$class_b_n_o08x.html#a5cc58139e4d5f0587b90e249ceb476f9" title="Queues a packet containing a command." alt="" coords="446,13,623,40"/>
<area shape="poly" id="edge2_Node000002_Node000003" title=" " alt="" coords="395,24,430,24,430,29,395,29"/>
<area shape="rect" id="Node000004" href="$class_b_n_o08x.html#a62c570ba96512f4d0d10b2594048de1f" title="Queues an SHTP packet to be sent via SPI." alt="" coords="671,13,831,40"/>
<area shape="poly" id="edge3_Node000003_Node000004" title=" " alt="" coords="624,24,656,24,656,29,624,29"/>
</map>
