<map id="BNO08x::wait_for_data" name="BNO08x::wait_for_data">
<area shape="rect" id="Node000001" title="Waits for a valid or invalid packet to be received or HOST_INT_TIMEOUT_MS to elapse." alt="" coords="465,43,619,69"/>
<area shape="rect" id="Node000002" href="$class_b_n_o08x.html#a367d525d1c0ba119b3dca3067bb5bccc" title="Checks if BNO08x has asserted interrupt and sent data." alt="" coords="248,16,408,43"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="449,47,408,42,408,37,450,42"/>
<area shape="rect" id="Node000004" href="$class_b_n_o08x.html#a11bb1b3fa44ad8f28c1492b5c07af886" title="Requests product ID, prints the returned info over serial, and returns the reason for the most resent..." alt="" coords="239,68,417,95"/>
<area shape="poly" id="edge3_Node000001_Node000004" title=" " alt="" coords="450,70,418,73,417,68,449,64"/>
<area shape="rect" id="Node000003" href="$class_b_n_o08x.html#ae6e875a27ae74ebed806ee1a4576845a" title="Runs full calibration routine." alt="" coords="5,5,191,48"/>
<area shape="poly" id="edge2_Node000002_Node000003" title=" " alt="" coords="232,31,191,30,191,25,233,26"/>
<area shape="rect" id="Node000005" href="$class_b_n_o08x.html#aea8e2c6dd7a2c9899479a7f39fe94798" title="Initializes BNO08x sensor." alt="" coords="35,72,161,99"/>
<area shape="poly" id="edge4_Node000004_Node000005" title=" " alt="" coords="223,86,161,87,161,82,223,80"/>
</map>
