<map id="BNO08x::enable_rotation_vector" name="BNO08x::enable_rotation_vector">
<area shape="rect" id="Node000001" title="Sends command to enable rotation vector reports (See Ref. Manual 6.5.18)" alt="" coords="5,88,172,131"/>
<area shape="rect" id="Node000002" href="$class_b_n_o08x.html#a41613e65ea9beef883184b7ef67affdd" title="Enables a sensor report for a given ID." alt="" coords="220,96,376,123"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="172,107,204,107,204,112,172,112"/>
<area shape="rect" id="Node000003" href="$class_b_n_o08x.html#af2951f6ea448af7cf7932fbfed9fec3c" title="Queues a packet containing a command with a request for sensor reports, reported periodically...." alt="" coords="432,29,591,72"/>
<area shape="poly" id="edge2_Node000002_Node000003" title=" " alt="" coords="348,93,416,74,418,79,350,98"/>
<area shape="rect" id="Node000004" href="$class_b_n_o08x.html#a2897a178bf2c53cd99df0d4570edf72e" title="Waits for data to be received over SPI, or HOST_INT_TIMEOUT_MS to elapse." alt="" coords="424,96,599,123"/>
<area shape="poly" id="edge4_Node000002_Node000004" title=" " alt="" coords="377,107,409,107,409,112,377,112"/>
<area shape="rect" id="Node000005" href="$class_b_n_o08x.html#a7cdeb849e728487de961cdfd4030c773" title="Waits for a queued packet to be sent or HOST_INT_TIMEOUT_MS to elapse." alt="" coords="424,147,599,173"/>
<area shape="poly" id="edge5_Node000002_Node000005" title=" " alt="" coords="358,121,438,140,437,145,357,126"/>
<area shape="poly" id="edge3_Node000003_Node000003" title=" " alt="" coords="471,29,469,19,476,10,490,5,512,3,535,5,548,11,546,16,533,10,512,8,492,10,479,15,474,21,476,28"/>
</map>
