<map id="BNO08x::data_proc_task" name="BNO08x::data_proc_task">
<area shape="rect" id="Node000001" title="Task responsible parsing packets. Executed when SPI task sends a packet to be parsed,..." alt="" coords="5,113,173,140"/>
<area shape="rect" id="Node000002" href="$class_b_n_o08x.html#a67a697595d6a4d4638a53c6b4a5ef0cd" title="Parses a packet received from bno08x, updating any data according to received reports." alt="" coords="221,113,377,140"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="173,124,205,124,205,129,173,129"/>
<area shape="rect" id="Node000003" href="$class_b_n_o08x.html#a4f66045a0528a0c17c52421ea51612e7" title="Parses received command report sent by BNO08x (See Ref. Manual 6.3.9)" alt="" coords="425,5,599,48"/>
<area shape="poly" id="edge2_Node000002_Node000003" title=" " alt="" coords="323,110,424,58,437,52,439,57,426,62,325,115"/>
<area shape="rect" id="Node000004" href="$class_b_n_o08x.html#a51b360d795563b55559f11efb40be36a" title="Sends packet to be parsed to meta data function call (frs_read_word()) through queue." alt="" coords="431,72,594,115"/>
<area shape="poly" id="edge3_Node000002_Node000004" title=" " alt="" coords="377,112,415,106,416,111,378,117"/>
<area shape="rect" id="Node000005" href="$class_b_n_o08x.html#a8d9db3e1b6208c2661e1c543deefa53d" title="Parses received input report sent by BNO08x." alt="" coords="440,139,585,181"/>
<area shape="poly" id="edge4_Node000002_Node000005" title=" " alt="" coords="378,136,424,144,423,149,377,142"/>
<area shape="rect" id="Node000006" href="$class_b_n_o08x.html#a29cfd7fc2816483ebebe9d55b677a036" title="Parses product id report and prints device info." alt="" coords="432,205,592,248"/>
<area shape="poly" id="edge5_Node000002_Node000006" title=" " alt="" coords="325,138,426,191,439,197,437,201,424,196,323,143"/>
</map>
