<map id="BNO08x::enable_ARVR_stabilized_game_rotation_vector" name="BNO08x::enable_ARVR_stabilized_game_rotation_vector">
<area shape="rect" id="Node000001" title="Sends command to enable ARVR stabilized game rotation vector reports (See Ref. Manual 6...." alt="" coords="5,80,178,139"/>
<area shape="rect" id="Node000002" href="$class_b_n_o08x.html#a41613e65ea9beef883184b7ef67affdd" title="Enables a sensor report for a given ID." alt="" coords="226,96,382,123"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="178,107,210,107,210,112,178,112"/>
<area shape="rect" id="Node000003" href="$class_b_n_o08x.html#af2951f6ea448af7cf7932fbfed9fec3c" title="Queues a packet containing a command with a request for sensor reports, reported periodically...." alt="" coords="438,29,597,72"/>
<area shape="poly" id="edge2_Node000002_Node000003" title=" " alt="" coords="354,93,422,74,424,79,356,98"/>
<area shape="rect" id="Node000004" href="$class_b_n_o08x.html#a2897a178bf2c53cd99df0d4570edf72e" title="Waits for data to be received over SPI, or HOST_INT_TIMEOUT_MS to elapse." alt="" coords="430,96,605,123"/>
<area shape="poly" id="edge4_Node000002_Node000004" title=" " alt="" coords="383,107,415,107,415,112,383,112"/>
<area shape="rect" id="Node000005" href="$class_b_n_o08x.html#a7cdeb849e728487de961cdfd4030c773" title="Waits for a queued packet to be sent or HOST_INT_TIMEOUT_MS to elapse." alt="" coords="430,147,605,173"/>
<area shape="poly" id="edge5_Node000002_Node000005" title=" " alt="" coords="364,121,444,140,443,145,363,126"/>
<area shape="poly" id="edge3_Node000003_Node000003" title=" " alt="" coords="477,29,475,19,482,10,496,5,518,3,541,5,554,11,552,16,539,10,518,8,498,10,485,15,480,21,482,28"/>
</map>
