<map id="BNO08x::enable_stability_classifier" name="BNO08x::enable_stability_classifier">
<area shape="rect" id="Node000001" title="Sends command to enable activity stability classifier reports (See Ref. Manual 6.5...." alt="" coords="5,88,174,131"/>
<area shape="rect" id="Node000002" href="$class_b_n_o08x.html#a41613e65ea9beef883184b7ef67affdd" title="Enables a sensor report for a given ID." alt="" coords="222,96,378,123"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="174,107,206,107,206,112,174,112"/>
<area shape="rect" id="Node000003" href="$class_b_n_o08x.html#af2951f6ea448af7cf7932fbfed9fec3c" title="Queues a packet containing a command with a request for sensor reports, reported periodically...." alt="" coords="434,29,593,72"/>
<area shape="poly" id="edge2_Node000002_Node000003" title=" " alt="" coords="350,93,418,74,420,79,352,98"/>
<area shape="rect" id="Node000004" href="$class_b_n_o08x.html#a2897a178bf2c53cd99df0d4570edf72e" title="Waits for data to be received over SPI, or HOST_INT_TIMEOUT_MS to elapse." alt="" coords="426,96,601,123"/>
<area shape="poly" id="edge4_Node000002_Node000004" title=" " alt="" coords="379,107,411,107,411,112,379,112"/>
<area shape="rect" id="Node000005" href="$class_b_n_o08x.html#a7cdeb849e728487de961cdfd4030c773" title="Waits for a queued packet to be sent or HOST_INT_TIMEOUT_MS to elapse." alt="" coords="426,147,601,173"/>
<area shape="poly" id="edge5_Node000002_Node000005" title=" " alt="" coords="360,121,440,140,439,145,359,126"/>
<area shape="poly" id="edge3_Node000003_Node000003" title=" " alt="" coords="473,29,471,19,478,10,492,5,514,3,537,5,550,11,548,16,535,10,514,8,494,10,481,15,476,21,478,28"/>
</map>
