<map id="BNO08x::wait_for_reset" name="BNO08x::wait_for_reset">
<area shape="rect" id="Node000001" title="Waits for SH2 HAL lib to detect reset or HOST_INT_TIMEOUT_DEFAULT_MS to elapse." alt="" coords="360,72,518,99"/>
<area shape="rect" id="Node000002" href="$class_b_n_o08x.html#a84a19cd1564f8d427394f137df54477d" title="Clears dynamic/motion engine calibration data and resets BNO08x device. See ref manual 6...." alt="" coords="150,5,312,48"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="374,70,308,51,310,46,375,65"/>
<area shape="rect" id="Node000004" href="$class_b_n_o08x.html#a28cd1c0b3477571d87133234e6358503" title="Hard resets BNO08x device." alt="" coords="161,72,301,99"/>
<area shape="poly" id="edge3_Node000001_Node000004" title=" " alt="" coords="344,88,301,88,301,83,344,83"/>
<area shape="rect" id="Node000006" href="$class_b_n_o08x.html#a973a1b1785f3302ee1b2702c6a27646e" title="Soft resets BNO08x device by sending RESET (1) command on &quot;device&quot; channel." alt="" coords="163,123,299,149"/>
<area shape="poly" id="edge5_Node000001_Node000006" title=" " alt="" coords="367,105,289,125,288,119,366,100"/>
<area shape="rect" id="Node000003" href="$_feature_tests_8cpp.html#a5258b4dbee44f7a6964ff93e378fd3fa" title=" " alt="" coords="5,13,102,40"/>
<area shape="poly" id="edge2_Node000002_Node000003" title=" " alt="" coords="134,29,102,29,102,24,134,24"/>
<area shape="rect" id="Node000005" href="$_feature_tests_8cpp.html#ad2587baeeb225c43d04e355166a29b18" title=" " alt="" coords="5,72,102,99"/>
<area shape="poly" id="edge4_Node000004_Node000005" title=" " alt="" coords="146,88,102,88,102,83,146,83"/>
<area shape="rect" id="Node000007" href="$_feature_tests_8cpp.html#abc6316f813506ff1114a4c50b5a72bdf" title=" " alt="" coords="5,123,102,149"/>
<area shape="poly" id="edge6_Node000006_Node000007" title=" " alt="" coords="148,139,102,139,102,133,148,133"/>
</map>
