<map id="BNO08x::clear_dynamic_calibration" name="BNO08x::clear_dynamic_calibration">
<area shape="rect" id="Node000001" title="Clears dynamic/motion engine calibration data and resets BNO08x device. See ref manual 6...." alt="" coords="5,48,168,91"/>
<area shape="rect" id="Node000002" href="$class_b_n_o08x.html#a96d47dd0f9aedfbe3f731f8ae76b2e85" title="Returns reason for previous reset via product ID report." alt="" coords="216,31,394,57"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="168,57,200,54,200,59,168,63"/>
<area shape="rect" id="Node000003" href="$class_b_n_o08x.html#a8e43dd50140f326cfb58e00399923e8c" title="Locks sh2 HAL lib to only allow the calling task to call its APIs." alt="" coords="449,5,611,32"/>
<area shape="poly" id="edge4_Node000001_Node000003" title=" " alt="" coords="130,45,171,29,215,16,271,8,328,5,434,7,434,12,328,10,272,14,216,21,172,34,132,50"/>
<area shape="rect" id="Node000004" href="$class_b_n_o08x.html#a2dbce689245a1b9968e3ea627d2b9a42" title="Unlocks sh2 HAL lib to allow other tasks to call its APIs." alt="" coords="442,56,618,83"/>
<area shape="poly" id="edge5_Node000001_Node000004" title=" " alt="" coords="168,67,426,67,426,72,168,72"/>
<area shape="rect" id="Node000005" href="$class_b_n_o08x.html#a6602374314c07e9f707c0a6d2234bf7e" title="Waits for SH2 HAL lib to detect reset or HOST_INT_TIMEOUT_DEFAULT_MS to elapse." alt="" coords="226,132,384,159"/>
<area shape="poly" id="edge6_Node000001_Node000005" title=" " alt="" coords="151,89,251,124,249,129,149,94"/>
<area shape="poly" id="edge2_Node000002_Node000003" title=" " alt="" coords="394,31,433,27,434,32,394,37"/>
<area shape="poly" id="edge3_Node000002_Node000004" title=" " alt="" coords="394,51,427,55,426,60,394,57"/>
</map>
