<map id="BNO08xSH2HAL::spi_open" name="BNO08xSH2HAL::spi_open">
<area shape="rect" id="Node000001" title="Opens SPI instance by waiting for interrupt." alt="" coords="5,43,186,69"/>
<area shape="rect" id="Node000002" href="$class_b_n_o08x_s_h2_h_a_l.html#a15b568922a498b988bd8b897b3ae2278" title="SPI wait for HINT sh2 HAL lib callback." alt="" coords="234,35,409,77"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="186,53,218,53,218,59,186,59"/>
<area shape="rect" id="Node000003" href="$class_b_n_o08x_s_h2_h_a_l.html#a0c4cc938180a997fb94c0c34c0dce07e" title="Hardware reset callback for sh2 HAL lib, toggle RST gpio." alt="" coords="457,5,637,48"/>
<area shape="poly" id="edge2_Node000002_Node000003" title=" " alt="" coords="409,42,441,38,442,43,410,47"/>
<area shape="rect" id="Node000005" href="$class_b_n_o08x.html#a69cf0da11a71f5ea40f9fddd598d06fc" title="Waits for HINT pin assertion or HOST_INT_TIMEOUT_DEFAULT_MS to elapse." alt="" coords="472,72,622,99"/>
<area shape="poly" id="edge4_Node000002_Node000005" title=" " alt="" coords="410,65,457,71,456,76,409,70"/>
<area shape="rect" id="Node000004" href="$class_b_n_o08x.html#a6711a624f7229f2eee51ee0a5bc87e67" title="Toggles reset gpio pin for hard reset of BNO08x device." alt="" coords="685,13,835,40"/>
<area shape="poly" id="edge3_Node000003_Node000004" title=" " alt="" coords="638,24,670,24,670,29,638,29"/>
</map>
