<map id="BNO08x::soft_reset" name="BNO08x::soft_reset">
<area shape="rect" id="Node000001" title="Soft resets BNO08x device by sending RESET (1) command on &quot;device&quot; channel." alt="" coords="5,56,141,83"/>
<area shape="rect" id="Node000002" href="$class_b_n_o08x.html#a96d47dd0f9aedfbe3f731f8ae76b2e85" title="Returns reason for previous reset via product ID report." alt="" coords="189,31,367,58"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="141,59,173,54,174,60,141,64"/>
<area shape="rect" id="Node000003" href="$class_b_n_o08x.html#a8e43dd50140f326cfb58e00399923e8c" title="Locks sh2 HAL lib to only allow the calling task to call its APIs." alt="" coords="422,6,584,32"/>
<area shape="poly" id="edge4_Node000001_Node000003" title=" " alt="" coords="97,53,138,33,188,16,244,8,301,4,407,6,407,11,301,9,245,13,189,21,140,38,99,58"/>
<area shape="rect" id="Node000004" href="$class_b_n_o08x.html#a2dbce689245a1b9968e3ea627d2b9a42" title="Unlocks sh2 HAL lib to allow other tasks to call its APIs." alt="" coords="415,56,591,83"/>
<area shape="poly" id="edge5_Node000001_Node000004" title=" " alt="" coords="141,67,399,67,399,72,141,72"/>
<area shape="rect" id="Node000005" href="$class_b_n_o08x.html#a6602374314c07e9f707c0a6d2234bf7e" title="Waits for SH2 HAL lib to detect reset or HOST_INT_TIMEOUT_DEFAULT_MS to elapse." alt="" coords="199,132,357,159"/>
<area shape="poly" id="edge6_Node000001_Node000005" title=" " alt="" coords="111,81,190,111,225,124,223,129,188,116,109,86"/>
<area shape="poly" id="edge2_Node000002_Node000003" title=" " alt="" coords="367,32,406,27,407,32,367,37"/>
<area shape="poly" id="edge3_Node000002_Node000004" title=" " alt="" coords="367,52,400,55,399,61,367,57"/>
</map>
