\doxysection{BNO08x\+Private\+Types Namespace Reference}
\hypertarget{namespace_b_n_o08x_private_types}{}\label{namespace_b_n_o08x_private_types}\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}}
\doxysubsubsection*{Classes}
\begin{DoxyCompactItemize}
\item 
struct \mbox{\hyperlink{struct_b_n_o08x_private_types_1_1bno08x__init__status__t}{bno08x\+\_\+init\+\_\+status\+\_\+t}}
\begin{DoxyCompactList}\small\item\em Holds info about which functionality has been successfully initialized (used by deconstructor during cleanup). \end{DoxyCompactList}\item 
struct \mbox{\hyperlink{struct_b_n_o08x_private_types_1_1bno08x__sync__ctx__t}{bno08x\+\_\+sync\+\_\+ctx\+\_\+t}}
\begin{DoxyCompactList}\small\item\em Holds context used to synchronize tasks and callback execution. \end{DoxyCompactList}\end{DoxyCompactItemize}
\doxysubsubsection*{Typedefs}
\begin{DoxyCompactItemize}
\item 
using \mbox{\hyperlink{namespace_b_n_o08x_private_types_a72315cafa76ff8c07f84f03fc6b36bc2}{bno08x\+\_\+cb\+\_\+list\+\_\+t}}
\begin{DoxyCompactList}\small\item\em Alias for vector type to contain both cb flavors. \end{DoxyCompactList}\item 
typedef struct BNO08x\+Private\+Types\+::bno08x\+\_\+init\+\_\+status\+\_\+t \mbox{\hyperlink{namespace_b_n_o08x_private_types_a2698bcb8153e67716b43ce3cccc0f31a}{bno08x\+\_\+init\+\_\+status\+\_\+t}}
\begin{DoxyCompactList}\small\item\em Holds info about which functionality has been successfully initialized (used by deconstructor during cleanup). \end{DoxyCompactList}\item 
typedef struct BNO08x\+Private\+Types\+::bno08x\+\_\+sync\+\_\+ctx\+\_\+t \mbox{\hyperlink{namespace_b_n_o08x_private_types_a67b3b4702d94bb4ba152a213feae944f}{bno08x\+\_\+sync\+\_\+ctx\+\_\+t}}
\begin{DoxyCompactList}\small\item\em Holds context used to synchronize tasks and callback execution. \end{DoxyCompactList}\end{DoxyCompactItemize}
\doxysubsubsection*{Enumerations}
\begin{DoxyCompactItemize}
\item 
enum \mbox{\hyperlink{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2f}{bno08x\+\_\+rpt\+\_\+bit\+\_\+t}} \+: Event\+Bits\+\_\+t \{ \newline
\mbox{\hyperlink{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fac0ff3fde600aac814ad76a4769515ae8}{EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+RV\+\_\+\+BIT}} = (1UL \texorpdfstring{$<$}{<}\texorpdfstring{$<$}{<} 0U)
, \mbox{\hyperlink{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fad39283f98adf7242b3b3ccf847c150cd}{EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+RV\+\_\+\+GAME\+\_\+\+BIT}} = (1UL \texorpdfstring{$<$}{<}\texorpdfstring{$<$}{<} 1U)
, \mbox{\hyperlink{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fab5d141bdda220e3fa0bd9eb0fe3f31b5}{EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+RV\+\_\+\+ARVR\+\_\+\+S\+\_\+\+BIT}} = (1UL \texorpdfstring{$<$}{<}\texorpdfstring{$<$}{<} 2U)
, \mbox{\hyperlink{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fab77588c26929a2d8dd8eeea883b905ca}{EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+RV\+\_\+\+ARVR\+\_\+\+S\+\_\+\+GAME\+\_\+\+BIT}} = (1UL \texorpdfstring{$<$}{<}\texorpdfstring{$<$}{<} 3U)
, \newline
\mbox{\hyperlink{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fa6835a63fb08379608cda0a108098aac7}{EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+GYRO\+\_\+\+INTEGRATED\+\_\+\+RV\+\_\+\+BIT}} = (1UL \texorpdfstring{$<$}{<}\texorpdfstring{$<$}{<} 4U)
, \mbox{\hyperlink{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fa728314f4744fc408c6b153e8fbb3feb4}{EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+GEOMAG\+\_\+\+RV\+\_\+\+BIT}} = (1UL \texorpdfstring{$<$}{<}\texorpdfstring{$<$}{<} 5U)
, \mbox{\hyperlink{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2faa5b9ffe097d1eb83a6a5a13871da0891}{EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+ACCELEROMETER\+\_\+\+BIT}} = (1UL \texorpdfstring{$<$}{<}\texorpdfstring{$<$}{<} 6U)
, \mbox{\hyperlink{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fa68851003c2b7df34c3acf882251c60e2}{EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+LINEAR\+\_\+\+ACCELEROMETER\+\_\+\+BIT}} = (1UL \texorpdfstring{$<$}{<}\texorpdfstring{$<$}{<} 7U)
, \newline
\mbox{\hyperlink{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fabd9e62157a0bc3dc38c3473d7bc2799f}{EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+GRAVITY\+\_\+\+BIT}} = (1UL \texorpdfstring{$<$}{<}\texorpdfstring{$<$}{<} 8U)
, \mbox{\hyperlink{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2faeb1961d7852ea305443610b2521aaea7}{EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+CAL\+\_\+\+GYRO\+\_\+\+BIT}} = (1UL \texorpdfstring{$<$}{<}\texorpdfstring{$<$}{<} 9U)
, \mbox{\hyperlink{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fa591c062247280798af0e40d6141614c6}{EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+UNCAL\+\_\+\+GYRO\+\_\+\+BIT}} = (1UL \texorpdfstring{$<$}{<}\texorpdfstring{$<$}{<} 10U)
, \mbox{\hyperlink{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fac1d15dddeab169b213c719e6b0fef32d}{EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+CAL\+\_\+\+MAGNETOMETER\+\_\+\+BIT}} = (1UL \texorpdfstring{$<$}{<}\texorpdfstring{$<$}{<} 11U)
, \newline
\mbox{\hyperlink{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2faa54d15cc17179a6840b9ec3f4e0038cb}{EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+UNCAL\+\_\+\+MAGNETOMETER\+\_\+\+BIT}} = (1UL \texorpdfstring{$<$}{<}\texorpdfstring{$<$}{<} 12U)
, \mbox{\hyperlink{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fad4482fb4fb6693a492584508691f2c77}{EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+TAP\+\_\+\+DETECTOR\+\_\+\+BIT}} = (1UL \texorpdfstring{$<$}{<}\texorpdfstring{$<$}{<} 13U)
, \mbox{\hyperlink{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fafb8f448edba339f37fdf794bd891f903}{EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+STEP\+\_\+\+COUNTER\+\_\+\+BIT}} = (1UL \texorpdfstring{$<$}{<}\texorpdfstring{$<$}{<} 14U)
, \mbox{\hyperlink{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fae138ae8422830982a470025d81c4be4b}{EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+STABILITY\+\_\+\+CLASSIFIER\+\_\+\+BIT}} = (1UL \texorpdfstring{$<$}{<}\texorpdfstring{$<$}{<} 15U)
, \newline
\mbox{\hyperlink{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fa94cddd1837a77bba5644543b1ad8b9e7}{EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+ACTIVITY\+\_\+\+CLASSIFIER\+\_\+\+BIT}} = (1UL \texorpdfstring{$<$}{<}\texorpdfstring{$<$}{<} 16U)
, \mbox{\hyperlink{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fad517d3ea5b1b259f20ed43e1fcf40e0c}{EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+SHAKE\+\_\+\+DETECTOR\+\_\+\+BIT}} = (1UL \texorpdfstring{$<$}{<}\texorpdfstring{$<$}{<} 17U)
, \mbox{\hyperlink{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fab7e6b36da354702880ff9118d45b6af2}{EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+RAW\+\_\+\+ACCELEROMETER\+\_\+\+BIT}} = (1UL \texorpdfstring{$<$}{<}\texorpdfstring{$<$}{<} 18U)
, \mbox{\hyperlink{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fadcfcdea69099869ebf7f246ff5b7e8bb}{EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+RAW\+\_\+\+GYRO\+\_\+\+BIT}} = (1UL \texorpdfstring{$<$}{<}\texorpdfstring{$<$}{<} 19U)
, \newline
\mbox{\hyperlink{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fab57a2ea711bebb4d4e031a0b449160c7}{EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+RAW\+\_\+\+MAGNETOMETER\+\_\+\+BIT}} = (1UL \texorpdfstring{$<$}{<}\texorpdfstring{$<$}{<} 20U)
, \mbox{\hyperlink{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fab5d7a8690f3b42637a52122d4269da10}{EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+CIRCLE\+\_\+\+DETECTOR\+\_\+\+BIT}} = (1UL \texorpdfstring{$<$}{<}\texorpdfstring{$<$}{<} 21U)
, \mbox{\hyperlink{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fa6bb054cdd31ded01373a4395889c84f1}{EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+ALL}}
 \}
\begin{DoxyCompactList}\small\item\em Bits for evt\+\_\+grp\+\_\+rpt\+\_\+en \& evt\+\_\+grp\+\_\+rpt\+\_\+data\+\_\+available. \end{DoxyCompactList}\item 
enum \mbox{\hyperlink{namespace_b_n_o08x_private_types_a59097f108831dd9860e17438d2976c1c}{bno08x\+\_\+tsk\+\_\+bit\+\_\+t}} \+: Event\+Bits\+\_\+t \{ \mbox{\hyperlink{namespace_b_n_o08x_private_types_a59097f108831dd9860e17438d2976c1ca272952aff639965d61f76664cb4fed15}{EVT\+\_\+\+GRP\+\_\+\+BNO08x\+\_\+\+TASKS\+\_\+\+RUNNING}}
, \mbox{\hyperlink{namespace_b_n_o08x_private_types_a59097f108831dd9860e17438d2976c1ca616d8458c1a9f54f9d99ba03a773ba41}{EVT\+\_\+\+GRP\+\_\+\+BNO08x\+\_\+\+TASK\+\_\+\+HINT\+\_\+\+ASSRT\+\_\+\+BIT}}
, \mbox{\hyperlink{namespace_b_n_o08x_private_types_a59097f108831dd9860e17438d2976c1caaddd073f2b8e89319909d7c61f220452}{EVT\+\_\+\+GRP\+\_\+\+BNO08x\+\_\+\+TASK\+\_\+\+RESET\+\_\+\+OCCURRED}}
, \mbox{\hyperlink{namespace_b_n_o08x_private_types_a59097f108831dd9860e17438d2976c1ca17f12f538e40746dbe8aafee08391fcc}{EVT\+\_\+\+GRP\+\_\+\+BNO08x\+\_\+\+TASK\+\_\+\+DATA\+\_\+\+AVAILABLE}}
 \}
\begin{DoxyCompactList}\small\item\em Bits for evt\+\_\+grp\+\_\+bno08x\+\_\+task. \end{DoxyCompactList}\end{DoxyCompactItemize}
\doxysubsubsection*{Variables}
\begin{DoxyCompactItemize}
\item 
static sh2\+\_\+\+Sensor\+Config \mbox{\hyperlink{namespace_b_n_o08x_private_types_a4f68e627c3c54e471ec83756b97924da}{default\+\_\+sensor\+\_\+cfg}}
\end{DoxyCompactItemize}


\doxysubsection{Typedef Documentation}
\Hypertarget{namespace_b_n_o08x_private_types_a72315cafa76ff8c07f84f03fc6b36bc2}\label{namespace_b_n_o08x_private_types_a72315cafa76ff8c07f84f03fc6b36bc2} 
\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!bno08x\_cb\_list\_t@{bno08x\_cb\_list\_t}}
\index{bno08x\_cb\_list\_t@{bno08x\_cb\_list\_t}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}
\doxysubsubsection{\texorpdfstring{bno08x\_cb\_list\_t}{bno08x\_cb\_list\_t}}
{\footnotesize\ttfamily using \mbox{\hyperlink{namespace_b_n_o08x_private_types_a72315cafa76ff8c07f84f03fc6b36bc2}{BNO08x\+Private\+Types\+::bno08x\+\_\+cb\+\_\+list\+\_\+t}}}

{\bfseries Initial value\+:}
\begin{DoxyCode}{0}
\DoxyCodeLine{\ etl::vector<etl::variant<BNO08xCbParamVoid,\ BNO08xCbParamRptID>,}
\DoxyCodeLine{\ \ \ \ \ \ \ \ \ \ \ \ CONFIG\_ESP32\_BNO08X\_CB\_MAX>}

\end{DoxyCode}


Alias for vector type to contain both cb flavors. 

\Hypertarget{namespace_b_n_o08x_private_types_a2698bcb8153e67716b43ce3cccc0f31a}\label{namespace_b_n_o08x_private_types_a2698bcb8153e67716b43ce3cccc0f31a} 
\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!bno08x\_init\_status\_t@{bno08x\_init\_status\_t}}
\index{bno08x\_init\_status\_t@{bno08x\_init\_status\_t}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}
\doxysubsubsection{\texorpdfstring{bno08x\_init\_status\_t}{bno08x\_init\_status\_t}}
{\footnotesize\ttfamily typedef struct BNO08x\+Private\+Types\+::bno08x\+\_\+init\+\_\+status\+\_\+t BNO08x\+Private\+Types\+::bno08x\+\_\+init\+\_\+status\+\_\+t}



Holds info about which functionality has been successfully initialized (used by deconstructor during cleanup). 

\Hypertarget{namespace_b_n_o08x_private_types_a67b3b4702d94bb4ba152a213feae944f}\label{namespace_b_n_o08x_private_types_a67b3b4702d94bb4ba152a213feae944f} 
\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!bno08x\_sync\_ctx\_t@{bno08x\_sync\_ctx\_t}}
\index{bno08x\_sync\_ctx\_t@{bno08x\_sync\_ctx\_t}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}
\doxysubsubsection{\texorpdfstring{bno08x\_sync\_ctx\_t}{bno08x\_sync\_ctx\_t}}
{\footnotesize\ttfamily typedef struct BNO08x\+Private\+Types\+::bno08x\+\_\+sync\+\_\+ctx\+\_\+t BNO08x\+Private\+Types\+::bno08x\+\_\+sync\+\_\+ctx\+\_\+t}



Holds context used to synchronize tasks and callback execution. 



\doxysubsection{Enumeration Type Documentation}
\Hypertarget{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2f}\label{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2f} 
\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!bno08x\_rpt\_bit\_t@{bno08x\_rpt\_bit\_t}}
\index{bno08x\_rpt\_bit\_t@{bno08x\_rpt\_bit\_t}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}
\doxysubsubsection{\texorpdfstring{bno08x\_rpt\_bit\_t}{bno08x\_rpt\_bit\_t}}
{\footnotesize\ttfamily enum \mbox{\hyperlink{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2f}{BNO08x\+Private\+Types\+::bno08x\+\_\+rpt\+\_\+bit\+\_\+t}} \+: Event\+Bits\+\_\+t}



Bits for evt\+\_\+grp\+\_\+rpt\+\_\+en \& evt\+\_\+grp\+\_\+rpt\+\_\+data\+\_\+available. 

\begin{DoxyEnumFields}{Enumerator}
\raisebox{\heightof{T}}[0pt][0pt]{\index{EVT\_GRP\_RPT\_RV\_BIT@{EVT\_GRP\_RPT\_RV\_BIT}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!EVT\_GRP\_RPT\_RV\_BIT@{EVT\_GRP\_RPT\_RV\_BIT}}}\Hypertarget{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fac0ff3fde600aac814ad76a4769515ae8}\label{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fac0ff3fde600aac814ad76a4769515ae8} 
EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+RV\+\_\+\+BIT&When set, rotation vector reports are active. \\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{EVT\_GRP\_RPT\_RV\_GAME\_BIT@{EVT\_GRP\_RPT\_RV\_GAME\_BIT}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!EVT\_GRP\_RPT\_RV\_GAME\_BIT@{EVT\_GRP\_RPT\_RV\_GAME\_BIT}}}\Hypertarget{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fad39283f98adf7242b3b3ccf847c150cd}\label{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fad39283f98adf7242b3b3ccf847c150cd} 
EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+RV\+\_\+\+GAME\+\_\+\+BIT&When set, game rotation vector reports are active. \\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{EVT\_GRP\_RPT\_RV\_ARVR\_S\_BIT@{EVT\_GRP\_RPT\_RV\_ARVR\_S\_BIT}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!EVT\_GRP\_RPT\_RV\_ARVR\_S\_BIT@{EVT\_GRP\_RPT\_RV\_ARVR\_S\_BIT}}}\Hypertarget{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fab5d141bdda220e3fa0bd9eb0fe3f31b5}\label{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fab5d141bdda220e3fa0bd9eb0fe3f31b5} 
EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+RV\+\_\+\+ARVR\+\_\+\+S\+\_\+\+BIT&When set, ARVR stabilized rotation vector reports are active. \\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{EVT\_GRP\_RPT\_RV\_ARVR\_S\_GAME\_BIT@{EVT\_GRP\_RPT\_RV\_ARVR\_S\_GAME\_BIT}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!EVT\_GRP\_RPT\_RV\_ARVR\_S\_GAME\_BIT@{EVT\_GRP\_RPT\_RV\_ARVR\_S\_GAME\_BIT}}}\Hypertarget{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fab77588c26929a2d8dd8eeea883b905ca}\label{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fab77588c26929a2d8dd8eeea883b905ca} 
EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+RV\+\_\+\+ARVR\+\_\+\+S\+\_\+\+GAME\+\_\+\+BIT&When set, ARVR stabilized game rotation vector reports are active. \\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{EVT\_GRP\_RPT\_GYRO\_INTEGRATED\_RV\_BIT@{EVT\_GRP\_RPT\_GYRO\_INTEGRATED\_RV\_BIT}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!EVT\_GRP\_RPT\_GYRO\_INTEGRATED\_RV\_BIT@{EVT\_GRP\_RPT\_GYRO\_INTEGRATED\_RV\_BIT}}}\Hypertarget{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fa6835a63fb08379608cda0a108098aac7}\label{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fa6835a63fb08379608cda0a108098aac7} 
EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+GYRO\+\_\+\+INTEGRATED\+\_\+\+RV\+\_\+\+BIT&When set, gyro integrator rotation vector reports are active. \\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{EVT\_GRP\_RPT\_GEOMAG\_RV\_BIT@{EVT\_GRP\_RPT\_GEOMAG\_RV\_BIT}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!EVT\_GRP\_RPT\_GEOMAG\_RV\_BIT@{EVT\_GRP\_RPT\_GEOMAG\_RV\_BIT}}}\Hypertarget{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fa728314f4744fc408c6b153e8fbb3feb4}\label{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fa728314f4744fc408c6b153e8fbb3feb4} 
EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+GEOMAG\+\_\+\+RV\+\_\+\+BIT&When set, geomagnetic rotation vector reports are active. \\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{EVT\_GRP\_RPT\_ACCELEROMETER\_BIT@{EVT\_GRP\_RPT\_ACCELEROMETER\_BIT}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!EVT\_GRP\_RPT\_ACCELEROMETER\_BIT@{EVT\_GRP\_RPT\_ACCELEROMETER\_BIT}}}\Hypertarget{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2faa5b9ffe097d1eb83a6a5a13871da0891}\label{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2faa5b9ffe097d1eb83a6a5a13871da0891} 
EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+ACCELEROMETER\+\_\+\+BIT&When set, accelerometer reports are active. \\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{EVT\_GRP\_RPT\_LINEAR\_ACCELEROMETER\_BIT@{EVT\_GRP\_RPT\_LINEAR\_ACCELEROMETER\_BIT}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!EVT\_GRP\_RPT\_LINEAR\_ACCELEROMETER\_BIT@{EVT\_GRP\_RPT\_LINEAR\_ACCELEROMETER\_BIT}}}\Hypertarget{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fa68851003c2b7df34c3acf882251c60e2}\label{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fa68851003c2b7df34c3acf882251c60e2} 
EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+LINEAR\+\_\+\+ACCELEROMETER\+\_\+\+BIT&When set, linear accelerometer reports are active. \\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{EVT\_GRP\_RPT\_GRAVITY\_BIT@{EVT\_GRP\_RPT\_GRAVITY\_BIT}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!EVT\_GRP\_RPT\_GRAVITY\_BIT@{EVT\_GRP\_RPT\_GRAVITY\_BIT}}}\Hypertarget{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fabd9e62157a0bc3dc38c3473d7bc2799f}\label{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fabd9e62157a0bc3dc38c3473d7bc2799f} 
EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+GRAVITY\+\_\+\+BIT&When set, gravity reports are active. \\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{EVT\_GRP\_RPT\_CAL\_GYRO\_BIT@{EVT\_GRP\_RPT\_CAL\_GYRO\_BIT}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!EVT\_GRP\_RPT\_CAL\_GYRO\_BIT@{EVT\_GRP\_RPT\_CAL\_GYRO\_BIT}}}\Hypertarget{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2faeb1961d7852ea305443610b2521aaea7}\label{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2faeb1961d7852ea305443610b2521aaea7} 
EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+CAL\+\_\+\+GYRO\+\_\+\+BIT&When set, calibrated gyro reports are active. \\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{EVT\_GRP\_RPT\_UNCAL\_GYRO\_BIT@{EVT\_GRP\_RPT\_UNCAL\_GYRO\_BIT}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!EVT\_GRP\_RPT\_UNCAL\_GYRO\_BIT@{EVT\_GRP\_RPT\_UNCAL\_GYRO\_BIT}}}\Hypertarget{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fa591c062247280798af0e40d6141614c6}\label{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fa591c062247280798af0e40d6141614c6} 
EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+UNCAL\+\_\+\+GYRO\+\_\+\+BIT&When set, uncalibrated gyro reports are active. \\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{EVT\_GRP\_RPT\_CAL\_MAGNETOMETER\_BIT@{EVT\_GRP\_RPT\_CAL\_MAGNETOMETER\_BIT}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!EVT\_GRP\_RPT\_CAL\_MAGNETOMETER\_BIT@{EVT\_GRP\_RPT\_CAL\_MAGNETOMETER\_BIT}}}\Hypertarget{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fac1d15dddeab169b213c719e6b0fef32d}\label{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fac1d15dddeab169b213c719e6b0fef32d} 
EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+CAL\+\_\+\+MAGNETOMETER\+\_\+\+BIT&When set, calibrated magnetometer reports are active. \\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{EVT\_GRP\_RPT\_UNCAL\_MAGNETOMETER\_BIT@{EVT\_GRP\_RPT\_UNCAL\_MAGNETOMETER\_BIT}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!EVT\_GRP\_RPT\_UNCAL\_MAGNETOMETER\_BIT@{EVT\_GRP\_RPT\_UNCAL\_MAGNETOMETER\_BIT}}}\Hypertarget{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2faa54d15cc17179a6840b9ec3f4e0038cb}\label{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2faa54d15cc17179a6840b9ec3f4e0038cb} 
EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+UNCAL\+\_\+\+MAGNETOMETER\+\_\+\+BIT&When set, uncalibrated magnetometer reports are active. \\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{EVT\_GRP\_RPT\_TAP\_DETECTOR\_BIT@{EVT\_GRP\_RPT\_TAP\_DETECTOR\_BIT}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!EVT\_GRP\_RPT\_TAP\_DETECTOR\_BIT@{EVT\_GRP\_RPT\_TAP\_DETECTOR\_BIT}}}\Hypertarget{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fad4482fb4fb6693a492584508691f2c77}\label{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fad4482fb4fb6693a492584508691f2c77} 
EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+TAP\+\_\+\+DETECTOR\+\_\+\+BIT&When set, tap detector reports are active. \\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{EVT\_GRP\_RPT\_STEP\_COUNTER\_BIT@{EVT\_GRP\_RPT\_STEP\_COUNTER\_BIT}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!EVT\_GRP\_RPT\_STEP\_COUNTER\_BIT@{EVT\_GRP\_RPT\_STEP\_COUNTER\_BIT}}}\Hypertarget{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fafb8f448edba339f37fdf794bd891f903}\label{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fafb8f448edba339f37fdf794bd891f903} 
EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+STEP\+\_\+\+COUNTER\+\_\+\+BIT&When set, step counter reports are active. \\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{EVT\_GRP\_RPT\_STABILITY\_CLASSIFIER\_BIT@{EVT\_GRP\_RPT\_STABILITY\_CLASSIFIER\_BIT}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!EVT\_GRP\_RPT\_STABILITY\_CLASSIFIER\_BIT@{EVT\_GRP\_RPT\_STABILITY\_CLASSIFIER\_BIT}}}\Hypertarget{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fae138ae8422830982a470025d81c4be4b}\label{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fae138ae8422830982a470025d81c4be4b} 
EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+STABILITY\+\_\+\+CLASSIFIER\+\_\+\+BIT&When set, stability classifier reports are active. \\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{EVT\_GRP\_RPT\_ACTIVITY\_CLASSIFIER\_BIT@{EVT\_GRP\_RPT\_ACTIVITY\_CLASSIFIER\_BIT}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!EVT\_GRP\_RPT\_ACTIVITY\_CLASSIFIER\_BIT@{EVT\_GRP\_RPT\_ACTIVITY\_CLASSIFIER\_BIT}}}\Hypertarget{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fa94cddd1837a77bba5644543b1ad8b9e7}\label{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fa94cddd1837a77bba5644543b1ad8b9e7} 
EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+ACTIVITY\+\_\+\+CLASSIFIER\+\_\+\+BIT&When set, activity classifier reports are active. \\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{EVT\_GRP\_RPT\_SHAKE\_DETECTOR\_BIT@{EVT\_GRP\_RPT\_SHAKE\_DETECTOR\_BIT}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!EVT\_GRP\_RPT\_SHAKE\_DETECTOR\_BIT@{EVT\_GRP\_RPT\_SHAKE\_DETECTOR\_BIT}}}\Hypertarget{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fad517d3ea5b1b259f20ed43e1fcf40e0c}\label{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fad517d3ea5b1b259f20ed43e1fcf40e0c} 
EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+SHAKE\+\_\+\+DETECTOR\+\_\+\+BIT&When set, shake detector reports are active. \\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{EVT\_GRP\_RPT\_RAW\_ACCELEROMETER\_BIT@{EVT\_GRP\_RPT\_RAW\_ACCELEROMETER\_BIT}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!EVT\_GRP\_RPT\_RAW\_ACCELEROMETER\_BIT@{EVT\_GRP\_RPT\_RAW\_ACCELEROMETER\_BIT}}}\Hypertarget{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fab7e6b36da354702880ff9118d45b6af2}\label{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fab7e6b36da354702880ff9118d45b6af2} 
EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+RAW\+\_\+\+ACCELEROMETER\+\_\+\+BIT&When set, raw accelerometer reports are active. \\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{EVT\_GRP\_RPT\_RAW\_GYRO\_BIT@{EVT\_GRP\_RPT\_RAW\_GYRO\_BIT}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!EVT\_GRP\_RPT\_RAW\_GYRO\_BIT@{EVT\_GRP\_RPT\_RAW\_GYRO\_BIT}}}\Hypertarget{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fadcfcdea69099869ebf7f246ff5b7e8bb}\label{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fadcfcdea69099869ebf7f246ff5b7e8bb} 
EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+RAW\+\_\+\+GYRO\+\_\+\+BIT&When set, raw gyro reports are active. \\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{EVT\_GRP\_RPT\_RAW\_MAGNETOMETER\_BIT@{EVT\_GRP\_RPT\_RAW\_MAGNETOMETER\_BIT}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!EVT\_GRP\_RPT\_RAW\_MAGNETOMETER\_BIT@{EVT\_GRP\_RPT\_RAW\_MAGNETOMETER\_BIT}}}\Hypertarget{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fab57a2ea711bebb4d4e031a0b449160c7}\label{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fab57a2ea711bebb4d4e031a0b449160c7} 
EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+RAW\+\_\+\+MAGNETOMETER\+\_\+\+BIT&When set, raw magnetometer reports are active. \\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{EVT\_GRP\_RPT\_CIRCLE\_DETECTOR\_BIT@{EVT\_GRP\_RPT\_CIRCLE\_DETECTOR\_BIT}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!EVT\_GRP\_RPT\_CIRCLE\_DETECTOR\_BIT@{EVT\_GRP\_RPT\_CIRCLE\_DETECTOR\_BIT}}}\Hypertarget{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fab5d7a8690f3b42637a52122d4269da10}\label{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fab5d7a8690f3b42637a52122d4269da10} 
EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+CIRCLE\+\_\+\+DETECTOR\+\_\+\+BIT&When set, circle detector reports are active. \\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{EVT\_GRP\_RPT\_ALL@{EVT\_GRP\_RPT\_ALL}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!EVT\_GRP\_RPT\_ALL@{EVT\_GRP\_RPT\_ALL}}}\Hypertarget{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fa6bb054cdd31ded01373a4395889c84f1}\label{namespace_b_n_o08x_private_types_ac53fb578d93a18b7a83903fc7a71dc2fa6bb054cdd31ded01373a4395889c84f1} 
EVT\+\_\+\+GRP\+\_\+\+RPT\+\_\+\+ALL&\\
\hline

\end{DoxyEnumFields}
\Hypertarget{namespace_b_n_o08x_private_types_a59097f108831dd9860e17438d2976c1c}\label{namespace_b_n_o08x_private_types_a59097f108831dd9860e17438d2976c1c} 
\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!bno08x\_tsk\_bit\_t@{bno08x\_tsk\_bit\_t}}
\index{bno08x\_tsk\_bit\_t@{bno08x\_tsk\_bit\_t}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}
\doxysubsubsection{\texorpdfstring{bno08x\_tsk\_bit\_t}{bno08x\_tsk\_bit\_t}}
{\footnotesize\ttfamily enum \mbox{\hyperlink{namespace_b_n_o08x_private_types_a59097f108831dd9860e17438d2976c1c}{BNO08x\+Private\+Types\+::bno08x\+\_\+tsk\+\_\+bit\+\_\+t}} \+: Event\+Bits\+\_\+t}



Bits for evt\+\_\+grp\+\_\+bno08x\+\_\+task. 

\begin{DoxyEnumFields}{Enumerator}
\raisebox{\heightof{T}}[0pt][0pt]{\index{EVT\_GRP\_BNO08x\_TASKS\_RUNNING@{EVT\_GRP\_BNO08x\_TASKS\_RUNNING}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!EVT\_GRP\_BNO08x\_TASKS\_RUNNING@{EVT\_GRP\_BNO08x\_TASKS\_RUNNING}}}\Hypertarget{namespace_b_n_o08x_private_types_a59097f108831dd9860e17438d2976c1ca272952aff639965d61f76664cb4fed15}\label{namespace_b_n_o08x_private_types_a59097f108831dd9860e17438d2976c1ca272952aff639965d61f76664cb4fed15} 
EVT\+\_\+\+GRP\+\_\+\+BNO08x\+\_\+\+TASKS\+\_\+\+RUNNING&When this bit is set it indicates the \doxylink{class_b_n_o08x}{BNO08x} tasks are running, it is always set to 1 for the duration of the \doxylink{class_b_n_o08x}{BNO08x} driver object. Cleared in the destructor for safe task deletion. \\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{EVT\_GRP\_BNO08x\_TASK\_HINT\_ASSRT\_BIT@{EVT\_GRP\_BNO08x\_TASK\_HINT\_ASSRT\_BIT}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!EVT\_GRP\_BNO08x\_TASK\_HINT\_ASSRT\_BIT@{EVT\_GRP\_BNO08x\_TASK\_HINT\_ASSRT\_BIT}}}\Hypertarget{namespace_b_n_o08x_private_types_a59097f108831dd9860e17438d2976c1ca616d8458c1a9f54f9d99ba03a773ba41}\label{namespace_b_n_o08x_private_types_a59097f108831dd9860e17438d2976c1ca616d8458c1a9f54f9d99ba03a773ba41} 
EVT\+\_\+\+GRP\+\_\+\+BNO08x\+\_\+\+TASK\+\_\+\+HINT\+\_\+\+ASSRT\+\_\+\+BIT&When this bit is set it indicates the \doxylink{class_b_n_o08x}{BNO08x} has asserted its host interrupt pin, thus an SPI transaction should commence. \\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{EVT\_GRP\_BNO08x\_TASK\_RESET\_OCCURRED@{EVT\_GRP\_BNO08x\_TASK\_RESET\_OCCURRED}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!EVT\_GRP\_BNO08x\_TASK\_RESET\_OCCURRED@{EVT\_GRP\_BNO08x\_TASK\_RESET\_OCCURRED}}}\Hypertarget{namespace_b_n_o08x_private_types_a59097f108831dd9860e17438d2976c1caaddd073f2b8e89319909d7c61f220452}\label{namespace_b_n_o08x_private_types_a59097f108831dd9860e17438d2976c1caaddd073f2b8e89319909d7c61f220452} 
EVT\+\_\+\+GRP\+\_\+\+BNO08x\+\_\+\+TASK\+\_\+\+RESET\+\_\+\+OCCURRED&When this bit is set it indicates the SH2 HAL lib has reset the IMU, any reports enabled by the user must be re-\/enabled. \\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{EVT\_GRP\_BNO08x\_TASK\_DATA\_AVAILABLE@{EVT\_GRP\_BNO08x\_TASK\_DATA\_AVAILABLE}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!EVT\_GRP\_BNO08x\_TASK\_DATA\_AVAILABLE@{EVT\_GRP\_BNO08x\_TASK\_DATA\_AVAILABLE}}}\Hypertarget{namespace_b_n_o08x_private_types_a59097f108831dd9860e17438d2976c1ca17f12f538e40746dbe8aafee08391fcc}\label{namespace_b_n_o08x_private_types_a59097f108831dd9860e17438d2976c1ca17f12f538e40746dbe8aafee08391fcc} 
EVT\+\_\+\+GRP\+\_\+\+BNO08x\+\_\+\+TASK\+\_\+\+DATA\+\_\+\+AVAILABLE&When this bit is set it indicates a report has been received for the user to read, cleared in data\+\_\+available() set/cleared in handle\+\_\+sensor\+\_\+report(). \\
\hline

\end{DoxyEnumFields}


\doxysubsection{Variable Documentation}
\Hypertarget{namespace_b_n_o08x_private_types_a4f68e627c3c54e471ec83756b97924da}\label{namespace_b_n_o08x_private_types_a4f68e627c3c54e471ec83756b97924da} 
\index{BNO08xPrivateTypes@{BNO08xPrivateTypes}!default\_sensor\_cfg@{default\_sensor\_cfg}}
\index{default\_sensor\_cfg@{default\_sensor\_cfg}!BNO08xPrivateTypes@{BNO08xPrivateTypes}}
\doxysubsubsection{\texorpdfstring{default\_sensor\_cfg}{default\_sensor\_cfg}}
{\footnotesize\ttfamily sh2\+\_\+\+Sensor\+Config BNO08x\+Private\+Types\+::default\+\_\+sensor\+\_\+cfg\hspace{0.3cm}{\ttfamily [inline]}, {\ttfamily [static]}}

{\bfseries Initial value\+:}
\begin{DoxyCode}{0}
\DoxyCodeLine{=\ \{\ }
\DoxyCodeLine{\ \ \ \ \ \ \ \ \ \ \ \ .changeSensitivityEnabled\ =\ \textcolor{keyword}{false},}
\DoxyCodeLine{\ \ \ \ \ \ \ \ \ \ \ \ .changeSensitivityRelative\ =\ \textcolor{keyword}{false},}
\DoxyCodeLine{\ \ \ \ \ \ \ \ \ \ \ \ .wakeupEnabled\ =\ \textcolor{keyword}{false},}
\DoxyCodeLine{\ \ \ \ \ \ \ \ \ \ \ \ .alwaysOnEnabled\ =\ \textcolor{keyword}{false},}
\DoxyCodeLine{\ \ \ \ \ \ \ \ \ \ \ \ .changeSensitivity\ =\ 0,}
\DoxyCodeLine{\ \ \ \ \ \ \ \ \ \ \ \ .reportInterval\_us\ =\ 0,}
\DoxyCodeLine{\ \ \ \ \ \ \ \ \ \ \ \ .batchInterval\_us\ =\ 0,}
\DoxyCodeLine{\ \ \ \ \ \ \ \ \ \ \ \ .sensorSpecific\ =\ 0\}}

\end{DoxyCode}
